[image: ]CARE INTERNATIONAL IN SOMALIA.
MOGADISHU OFFICE. 
	DATE: October 12, 2021
	
Company Name: _______________________________________Telephone_______________

Bid Document for the Rehabilitation and reinforcement of EMIS Operationalization centre, two staircase rooms and roof at HQ the Ministry of Education Culture and Higher Education in Mogadishu.
Below is the summery total quote for the items.

	  Bill of Quantities Date:                                                                                                             

	P.T
	Bill of Quantity for the Rehabilitation and reinforcement of EMIS Operationalization centre, two staircase rooms and roof at HQ the Ministry of Education Culture and Higher Education in Mogadishu.    

	ITEM
	DESCRIPTION OF WORK
	Quantity
	Unit
	PRICE (USD)
	TOTAL AMOUNT (USD)

	Important Notes: The contractor should visit the site to verify the amount of work before estimating & signing the contract. a sample of all materials should be reviewed and approved by Supervisor Engineer in charge prior to implementation, all works shall be carried out according to specification, condition, and as directed by the engineer. In case of any difference between BOQ, and actual work the instruction of site Engineer will govern, no extra cost to project. After all work is completed, the site must be cleaned from all debris and neglected materials must be removed to approved dump site, If contractor fails to clean the site from debris, client shall appoint 3rd party contractor and back charge the cost to fencing contractor.

	1.00
	MOBILIZATION WORK
	 
	 
	 
	 

	1.10
	CONTRACTOR'S SITE ESTABILISHMENT of Transportation and establishing of all personnel, tools, equipment, materials and all other necessary items for the execution of the 'work.
	Lms
	1.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	2.00
	Staircase room and parapet wall
	 
	 
	 
	 

	2.02
	Provide and Construct precast hollow cement blocks wall having 200mm thick wall in standard precast hollow cement blocks with minimum compressive strength of 35kg/sqcm bedded and jointed in cement and sand (1:3) mortar proportion ratio, Corner cement block should be good dressed and jointed to correct angles. All gaps in between cement blocks should be filled with cement sand mortar well mixed, reinforced with and including 25mm wide x 20 gauge hoop iron at every alternate course as described in: Note before extenting the wall prepare Bonding ties use 20 gauge  hoop iron ties 25mm wide bent and tacked into formwork with one end cast into morter jiont of walling
	SQM
	150.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	3.00
	Plastering And Painting Work
	 
	 
	 
	 

	3.01
	Providing and rendering 12 mm thick cement plaster in cement mortar 1:4 (1 cement :4 fine sand) on external/internal surfaces of brick walls, columns, beams and inside surface/slabs composed of a bond coat (1 cement: 2 sand,) base coat 1: 4, and finish coat 1: 5 with ordinary Portland cement and sand as specified, The price also includes material and labor and subject to Engineer Approval..
	SQM
	2,125.0
	 
	 

	N.B
	Note: The contructor should allow in his pricing that the client may use as many diference colour or combination colors to meet and approved color scheme. no hand made color mix is allowed, beforey any color the contractor has to prepare a color sample 1x 1m on site for each color asked by the enginer. you should also keep in mind that the owner has to right to chose any color or combination no price difference will be measures for any color variation done.

	3.02
	Prepare and apply one coat of primer, two undercoats of brilliant white emulsion paint and two finishing coats of first quality brilliant white Silk Vinyl emulsion paint of approved colour and approved manufacturer, to all int/external walls and inside surface slap as per direction of engineer in charge. Paint shall be from approved colour with approved manufacturer 
	SQM
	2,605.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	4.00
	DOOR & WINDOWS COMPONENTS
	 
	 
	 
	 

	4.01
	Supply and install, by a qualified supplier, natural aluminium casement sliding windows, overall size (120cm L x 100cm H ) glazed in bronze 6mm glass, well secured in rubber and fitted on window jambs with brass screws. 
	NO
	15.0
	 
	 

	 
	Supply and install Pvc fixed windows complete with opening accessories and permanent vents for the full width of window as detailed including cuMBng and 4mm thick toughened glazing fixing lugs to wood frame and pointing all round frames. Window size 1000mm x 1300mm high.
	No
	8.0
	 
	 

	4.02
	Supply and install aluminium casement windows complete with opening accessories and permanent vents for the full width of window as detailed including cuMBng and 4mm thick toughened glazing fixing lugs to wood frame and pointing all round frames. Window size 600mm x 500mm high.
	NO
	3.0
	 
	 

	4.03
	Burglar Proofing: Burglar Proofing galvanized mild steel grille framed with 40 x 25 x 3 mm thick R.H.S sections including assembly and fixing to opening cutting and pinning lugs to concrete or blockwork and bedding frame in cement sand mortar (1:4), 600square x bars1500mmlap-jointedwith diamond at 100mm patterned centresY16 for 14 windows as per direction of engineer.
	SQM
	50.0
	 
	 

	4.04
	Providing and installing Shatter Resistance plastic Film to the glass windows for only internal sides, the quality of the plastic should be checked before it is sealed.
	SQM
	50.0
	 
	 

	4.05
	Providing and fixing teak wooden doors first quality of Size 1000mm X 1200 mm made out of 4mm thick, (Manufuctuted Turky) with all necessary frames, sub frames, fixing, fittings, accessories weather stripping and hardware as per specifications and engineer's instructions.
	NO
	13.0
	 
	 

	4.06
	Provide and fix 50mm thick hard wood panel mahogany doors Single leaf openable door overal size 900 x 2100mm high overall; 
	NO
	3.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	5.00
	Ceramic Floor Tiles & Skirting 
	 
	 
	 
	 

	5.01
	Providing and laying 1st quality white Non-slip ceramic floor tile in sizes 6000mm x 6000mm x 60 mm thickness (UAE product) in toilets, the corridor floor and rooms of approved make, in all colors and shades, laid on 20mm thick cement mortar 1:4 (1 cement: 4 coarse sand), including grouting the joints with white cement and matching pigments etc., complete Calculation per m2. the item included Tile skirting for all collective rooms and corridor.
	SQM
	638.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	6.00
	PLUMBING AND SANITARY FIXTURES
	 
	 
	 
	 

	NB
	Supply and install the following high-quality plumbing, sanitary appliances and fixtures as approved by the Engineer, Complete with all accessories including cutting & making good wall & floor wherever required, all piping must be ceased and concealed in walls.

	6.01
	Supply and fix High quality European‐type ceramic W.C suite consisting of pan trap and cistern with seat and cover as ‘Duravit’ or any other quality equivalent, with minimum 9-liter plastic double action flushing cistern, price including fittings, brackets, repair walls etc.‐white with plastic seat & lid.
	NO
	3.0
	 
	 

	6.02
	White vitreous ceramic wash handbasin with single Wash Basin tap, chain, 32mm plastic bottle trap and fixing brackets including connection to water supply and waste.
	NO
	1.0
	 
	 

	6.05
	Providing and fixing toilet Paper Holder and fixing a single Muslim Shower, towel rails, ring, & soap dish. Note: these items are needed per toilet x three bathroom 
	Lms
	3.0
	 
	 

	6.07
	Amend, providing and fixing PVC plumbing pipe having size of 1/2, and 3" P.V.C drainage pipes including all necessary bends connections, complete with PVC fittings and clamps i/c making good concealed all pipes to the walls (excluding fittings, refilling, clamps & repair walls Internal piping) this price also including painting with anti-corrosive bitumastic paint, cutting chases and making good the wall.
	lms
	1.0
	 
	 

	4.80
	Testing and Commissioning Rate to include all tastings to be done all plumbing systems and all other fittings and accessories to complete in all respects as per directed by the Engineer In charge. 
	lms
	1.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	7.00
	STAIRCASE 
	 
	 
	 
	 

	7.01
	Approved murram filling to make up levels, well rammed, watered and consolidated in 1000mm thick layers complete. Half of the back filling material comes out the previous demolished structures
	M3
	20.0
	 
	 

	7.02
	Supply and cast ready mix reinforced concrete B(250) kg/cm2 for the ground slab on stair case steps and landings 10cm thick with steel mesh 8mm diameter every 20cm.as per  site condition and specifications 
	M3
	16.0
	 
	 

	7.03
	Staircase finishes: Rendering in 1:3 cement screeds, backings, beds etc 32mm bed finished to receive ceramic tiles to landing (m.s), 20mm thick to receive treads, 300mm wide ditto, 12mm thick to receive risers, 150mm high ditto.

	M3
	30.0
	 
	 

	7.04
	Construction of stairs room top slap: Supply and cast ready mix reinforced concrete B(250) kg/cm2 for the top slab 10cm thick, Stairs to be reinforced with RO12 to 10cm as a structural reinforcement and Ø6 to 20cm as the transverse beams. Beams at the outer wall; Stirrups to be done out of smooth armature Ø6 at every 20 cm. 
	Me 
	1.2
	 
	 

	7.05
	Supply and lay Granite (rozbita) for staircases size120 cm length 33 cm wide x 3cm thick, risers size 120 cm length 15 cm high x 2 cm thick) laid on 2cm thick cortar bed. The price including skirting 2cm thick on both sides, and final polishing as per specifications, drawings and supervisor engineer instructions. RISE AND WIDTH CALCULTED FOR ONE PIECE,
	PIECE
	102.0
	 
	 

	7.06
	Staircase railing with one 50 mm dia and two 25 mm dia medium MS pipe horizontal rails and 32 mm dia, 900 mm high medium MS pipe balusters spaced at 600 mm c/c in the veranda and one on alternate tread of the staircase, including 10X10mm MS Solid bar combination and painting with two coats of anti-corrosive metal primer and two coats of enamel paint, all complete as per specifications/instruction, (Calculation of lm is calculated one step both trade and Rise)
 
	Lms
	30.0
	 
	 

	7.07
	Supply, assemble, Fabricate and fix the following purpose-made steel section Panel metal door comprising of 50x50x6mm steel angle framing fully welded and mitred at corners all round 1 No. 50x25x3mm RHS intermediate horizontal rails; ends  welded and angles cut, mitred and welded; 3mm thick steel plate panels on both side three hinges leaf; tower and barrel bolts with  bolt guides locking cleats with padlock eyes; all welding ground to smooth finish; four panel per leaf.  Ditto 2600 x 3100mm high overall; single leave 
	No
	1.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	8.00
	ELECTRICAL INSTALLATIONS AND SERVICES
	 
	 
	 
	 

	N.B
	Work in connection with electrical installations: Delivery and laying, connecting, putting under voltage of cables, power distribution box, lighting cabinet and sockets and forming chassis holes of approved type. The cables are laid by air construction on the walls construction according then concealed by mortar. All put into boxes and put under voltage. Before purchasing and cutting lengths should be checked on the site by measuring routes. Wiring and installation (including supply of all materials) of the light points using approved type PVC insulated PVC sheathed 1.5 mm² copper cables and 2.5mm² earth cable drawn through securely fixed concealed PVC conduit, to the walls and slab surfaces Socket outlet points

	8.01
	Supply & installation of 40W Ceiling mounted circular lights, complete in all respects as per directed by the Engineer In charge. 
	Nos
	40.0
	 
	 

	8.02
	Socket outlets: Supply & installation of 15A shuttered switched double socket outlet to comply with BS 1363. Rate to include for Wiring (including supply of all material required) of 15A Socket (Two Gang) outlets using approved type 2.5mm2 Cu/PVC/PVC, 2C cable & 2.5mm2 earth cable drawn through securely fixed concealed PVC conduit.
	Nos
	42.0
	 
	 

	8.03
	Switch point: Supply and & fixing modular 5/6 Amp one way switch, complete with connection, testing & commissioning etc. 
	No
	30.0
	 
	 

	8.04
	Checking and testing electrical wires in all room, and it may be made some changes of 15A shuttered switched double socket outlet. 
	Lms
	1.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	9.00
	Air conditioning
	 
	 
	 
	 

	9.01
	"Provision, installation and commission air conditioning units-18000 BTU split-type AC- Super general. This item and its cost includes BTU split-type AC unit including all required accessories, fittings, electric cabling copper pipes, fixings, etc. to the functioning state to full satisfaction of Engineer"
	No
	14
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	10.00
	Top Floor Finishing
	 
	 
	 
	 

	10.01
	Slope preparations for final paved areas, Average 120mm thick to make up levels, Allow for water drainage proper angle to move, using proper slope as per direction of the Building.
	M3
	68.0
	 
	 

	10.02
	Providing water proofing treatment to top floors by using bituminous waterproof coating followed by brushed of minimum 1 mm thickness, including surface preparation, curing, etc. complete in accordance with directions, and specifications
	SQM
	560.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	11.00
	CABINET STORAGE -IT ROOM 
	 
	 
	 
	 

	11.01
	Providing & fixing overhead modular cabinet storage, made of 19 mm thick block board with shutters and shelves, 12mm thick plywood all outer sides & surfaces (all visible area) shall be finished with 4mm thick teak veneer. Sides & bottom shall be made of 19 mm thick plywood & back side shall be made of 6mm thick plywood; intermediate shelf shall be made of 19mm thick plywood. The cabinet has group locks, hinges, stopper, magnate, handles of approved make & quality and provided S.S. satin finished handle of approved shape & size Complete. The work shall be measured based on area of front elevation of each storage unit. The rate to include all materials, labor, transport, delivered and placed in position at site of work. 
	SQM
	23.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	12.00
	Level Ground yard
	 
	 
	 
	 

	12.01
	Surface preparation Clean & remove dust, dirt, loose particles and unsound substrate, well compacted and well-watered in layers compaction to BS 95% compacting by rolling, The work shall be completed according to the technical guidance of engineer and the client approval.
	SQM
	200.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	13.00
	SITE CLEANING AFTER COMPILATION OF THE WORK 
	 
	 
	 
	 

	13.01
	Environmental Management: Upon practical completion thoroughly clean out all area by washing all floors, removing paint stains, motor droppings, and clear site completely of all debris all in good order in handing over.
	Lms
	1.0
	 
	 

	 
	Sub Total
	 
	 
	 
	 

	 
	Total Summary for collective sum
	 





SELECTION CRITERIA FOR THIS BID IS AS BELOW.
1. Valid Trade License company registration certificates from Ministry of Commerce at FGS
2. Updated company profile with your company contacts details and physical address and all pertinent information, 
3. Proof of tax clearance from the government.
4. Proof of Similar works experience such former contracts/purchase orders.
5. Detail delivery time (Attach work plan)

Send to procurement@moe.gov.so your complete and stamped bid documents marking in the subject line Bid Document for the Rehabilitation and reinforcement of EMIS Operationalization centre, two staircase rooms and roof at HQ the Ministry of Education Culture and Higher Education in Mogadishu. on or before   October 25, 2021, 16:30. No responses will be accepted after this date.
Note: if you send to or copy your bid response to any other email your bid documents will be automatically disqualified.
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